Zone Measurement Read

KByte/s

Test started: 04-26-04 22:04:19, test version: $Id: h2bench.c,v 3.6 2002/10/31 14:06:35 bo Exp $/Win32, file name ’fb_mv-md-4G’ command line: h2benchw -english -w fb_mv-md-4G -c 0 -z -s 1 timer resolution: 0.279 μs, 3.580 MHz, timer statistics: 5137 calls, min 997.89 μs, average 186925.14 μs, max 1124211.88 μs

Carry Computer FotoBar BSDR USB 2.0